From fc552b1e5c503c530763e40d2b83df55c5c2e9a3 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 25 Mar 2020 20:58:35 +0100
Subject: [PATCH] rpi-eeprom-update: change default include path
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 rpi-eeprom-update | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

--- a/rpi-eeprom-update
+++ b/rpi-eeprom-update
@@ -6,8 +6,8 @@ set -e
 
 script_dir=$(cd "$(dirname "$0")" && pwd)
 
-if [ -f /etc/default/rpi-eeprom-update ]; then
-   . /etc/default/rpi-eeprom-update
+if [ -f /etc/bcm27xx-eeprom.conf ]; then
+   . /etc/bcm27xx-eeprom.conf
 fi
 
 LOCAL_MODE=0
@@ -436,7 +436,7 @@ checkDependencies() {
       echo "Run with -h for more information."
       echo
       echo "To enable flashrom programming of the EEPROM"
-      echo "Add these the following entries to /etc/default/rpi-eeprom-update"
+      echo "Add these the following entries to /etc/bcm27xx-eeprom.conf"
       echo "RPI_EEPROM_USE_FLASHROM=1"
       echo "CM4_ENABLE_RPI_EEPROM_UPDATE=1"
       echo 
@@ -523,7 +523,7 @@ The system should then boot normally.
 
 If /boot does not correspond to the boot partition and this
 is not a NOOBS system, then the mount point for BOOTFS should be defined
-in /etc/default/rpi-eeprom-update by defining the BOOTFS variable.
+in /etc/bcm27xx-eeprom.conf by defining the BOOTFS variable.
 
 A backup of the current EEPROM config file is written to ${FIRMWARE_BACKUP_DIR}
 before applying the update.
@@ -555,7 +555,7 @@ Options:
    -u Install the specified VL805 (USB EEPROM) image file.
 
 Environment:
-Environment variables should be defined in /etc/default/rpi-eeprom-update
+Environment variables should be defined in /etc/bcm27xx-eeprom.conf
 
 EEPROM_CONFIG_HOOK
 
@@ -627,7 +627,7 @@ must first be enabled by removing ENABLE
 via usbboot.
 
 After enabling self-update set the CM4_ENABLE_RPI_EEPROM_UPDATE=1 environment
-variable or define it in /etc/default/rpi-eeprom-update.
+variable or define it in /etc/bcm27xx-eeprom.conf.
 
 N.B. If there is a power failure during SELF_UPDATE the EEPROM write may fail and
 usbboot must be used to flash the bootloader EEPROM. SELF_UPDATE is not recommended
